**LED Floodlight Specification:**

|  |  |
| --- | --- |
| Item Type | 100W LED Floodlight |
| LED Type | Epistar/Bridgelux/Cree |
| Power | 100W |
| Lamp Luminous Flux | 7000-9000lm |
| Lamp Luminous Effciency | 70-90lm/W |
| CRI | ≥75Ra |
| Color Temperature | 2700~3500K(WW),4000~4500K(NW),6000~7000K(CW) |
| Beam Angle | 120-140 degree |
| IP Grade | IP65 |
| Input Voltage | AC85-265V |
| Frequency | 50/60HZ |
| Lamp Body Material | Aluminum Alloy |
| Life Time | ≥35000hours |
| Working Temperature | -20°C~+45°C |
| Shell Color | Grey or Black |
| Dimension | 290\*290\*90mm |
| Appliance Class | Class I |
| Certification | CE, RoHS, FCC |
| Warranty | 2 years |