**CONSTRUCTION OF HULHUMALE’ POLICE STATION (NEIGHBOURHOOD 1)**

**ADDITIONAL INFORMATION**

1. AutoCad drawings can be accessed from the drop box link below.

https://www.dropbox.com/sh/oueimy9e4su3dnu/AADvhEuKe-cHIhceAtzP4vnKa?dl=0

1. Firefighting exit sign board should be on all floors stair lobby area.
2. Boundary wall structural details are provided separately in boundary wall details.
3. Air-condition should be included, and is included in BOQ.
4. Damp proof membrane is included in BOQ and the quantity is 501.25 m2
5. There is no RCC rainwater tank.
6. There is no server room. There will be a wall mount network switch with rack on first floor Investigation room and second floor admin room.
7. For firefighting only CO2 and H2O shall be fixed on each floor.
8. Glass blocks rates can be included on masonry wall.