**ADDITIONAL INFORMATION**

**Project: Construction of R.Angolhitheem Health Center**

**Please be informed that:**

1. Interior & Exterior Plastering: 18mm thick.

a. Block making: Local sand shall be used (mix ratio 1:4)

b. River sand shall be used for bedding motar & Plastering. Manufactured sand cannot be used.

2. Interior Ceiling: Gypsum Board with G.I frame as per manufacture’s Instruction. (Hidden frame)

3. The following drawings are attached with this amendment

a. Revised Electric Layout (AC Outdoor unit locations)

b. Hydraulics and drainage drawings

c. Septic tank location (Site plan attached)

d. Ground water well location (Site plan attached)

e. Water tank location (Site plan attached)

4. Material Storage shall be arranged within health center premises, staff accommodation could be arranged within health center premises if space available (if the services of health center is not interrupted).

5. No demolition works are to be carried out. Proposed building area has been cleared of any existing structure.

6. Three phase armored cable to be laid from nearest Distribution board (of power station) to the building (contractor shall check the distance from power station’s Distribution board to Health center before bidding)

7. No electric main panel board is required, only house meter and distribution board is required (all are three phase).

8. Supply and complete installation of 5000 Liters HDPE (Sintex or Equivalent) Rain water storage tanks as per drawing. (This item includes laying foundation of the storage tank bed and roofing works as per drawing)

9. Construction of overhead tank tower as per drawing and installation of overhead storage tank (2500L HDPE tank – sintex or equivalent).