# Additional Informations for Construction of Sh.Noomara Council Office.

* Nearest Electric Distribution box is located in 220 Ft.
* There are 6 trees (Dhiggaa) to be removed (cut down) from site.
* There is space to make the temporary accommodation and storage space to keep the equipment’s and material at behind the site.
* Ground water could be used to make block for masonry work.
* Please find the attached final BOQ and Drawing for Sh. Noomaraa council. The following are the clarifications asked.
  + Portico and guard post roof slab not included in the boq.

130mm  refer boq

* + Cleaner room door sizes not given in the drawing.

included in the boq and Drawing

* + Tea room sink not included in the boq.

included in the boq

* + Toilet wash basin qty different between boq and drawing.

NO, its ok in the boq and the drawing

* + AC point given in the drawing but not in the boq.

12 AC

* + TV. Phone, network sock given in the boq but wiring point and cable not included.

Yes, wiring points given in the drawing, contractors have to find the cable lengths.

* + Steps not included in the boq.

Give in the addition bill if there is any steps

* + Gutter not given in the boq.

included in the boq

* + Fascia board not given in the boq.

included in the boq

* + Ridge beam and purles size different between drawing and boq.

Battens size is ok 50mmx 50mm, and Ridge beam size is 200x50mm

* + Timber strip not given in the boq.

included in the boq

* + Compound wall drawing given but not in the BOQ  
    included in the BOQ.